sw_checklist:BEFORE STARTING CHECKLIST
sw_rcolsize:80
sw_item:Parking Brake|SET:sim/flightmodel/controls/parkbrake:>0
sw_item:Doors|CLOSED
sw_item:Battery|ON (GPU to recharge):sim/cockpit2/electrical/battery_on:1
sw_item:Ground Power|GPU Disconnected
sw_item:Generators|ON:(sim/cockpit/electrical/generator_on[0]:1)&&(sim/cockpit/electrical/generator_on[1]:1)
sw_item:Nav Lights, Beacon|ON:(sim/cockpit/electrical/nav_lights_on:1)&&(sim/cockpit/electrical/beacon_lights_on:1)
sw_item:Cabin signs|ON:(sim/cockpit/switches/fasten_seat_belts:1)&&(sim/cockpit/switches/no_smoking:1)
sw_item:Ignition master|ON (Pushed in)
sw_item:Magnetos|OFF:(sim/cockpit/engine/ignition_on[0]:0)&&(sim/cockpit/engine/ignition_on[1]:0)
sw_remark: or ON for hot start (oil temp >40°)
sw_item:Fuel Quantity|CHECKED all 4 tanks
sw_remark:(Turn Fuel Quantity Selector and check all 4 tanks.)
sw_item:Fuel Selectors|LM, RM:(sim/cockpit2/fuel/fuel_tank_selector_left:1)&&(:sim/cockpit2/fuel/fuel_tank_selector_right:3)
sw_item:Carb heat|COLD:(sim/cockpit2/engine/actuators/carb_heat_ratio[0]:0)&&(sim/cockpit2/engine/actuators/carb_heat_ratio[1]:0)
sw_item:Trim|ZERO:sim/flightmodel2/controls/elevator_trim:0
sw_item:Cowl Flaps|OPEN:(sim/flightmodel/engine/ENGN_cowl[0]:1)&&(sim/flightmodel/engine/ENGN_cowl[1]:1)
sw_item:Mixture|IDLE CUTOFF:(sim/flightmodel/engine/ENGN_mixt[0]:0.0)&&(sim/flightmodel/engine/ENGN_mixt[1]:0.0)
sw_item:Throttle|Idle:(sim/cockpit2/engine/actuators/throttle_ratio[0]:0)&&(sim/cockpit2/engine/actuators/throttle_ratio[1]:0)
sw_item:Propeller Control|Fine:(sim/flightmodel/engine/ENGN_prop[0]:<86)&&(sim/flightmodel/engine/ENGN_prop[1]:<86)
sw_item:Flight Controls|FREE 
sw_remark:Push Yoke - full forward, then full back, full left and full right.
sw_remark:Rudder - full left and full right.

sw_checklist:ENGINE START (COCKPIT)
sw_remark:     -- Standard sequence is Right-Left (2-1) --
sw_remark:RIGHT ENGINE
sw_item:Fuel Pump |ON:sim/cockpit/engine/fuel_pump_on[1]:1
sw_item:Throttle|CRACKED 10%-15%:(sim/cockpit2/engine/actuators/throttle_ratio[1]:>0.09)&&(sim/cockpit2/engine/actuators/throttle_ratio[1]:<0.16)
sw_item:Propeller Control (Pitch)|FULL FORWARD (HIGH RPM):(sim/flightmodel/engine/ENGN_prop[1]:>150)
sw_item:Mixture|AUTO RICH:(sim/flightmodel/engine/ENGN_mixt[1]:>0.73)&&(sim/flightmodel/engine/ENGN_mixt[1]:<0.80)
sw_item:Starter|ENGAGE (count blades):sim/cockpit2/engine/actuators/starter_hit[1]:1
sw_item:Magnetos|BOTH:sim/cockpit/engine/ignition_on[1]:3
sw_item:Primer|press repeatedly or keep pressed until engine fires:sim/cockpit2/engine/actuators/primer_on[1]:1
sw_remark:(Repeat starting procedure for left engine.)

sw_checklist:BEFORE TAXI CHECKLIST
sw_item:Inverters|ON
sw_item:Avionics|ON
sw_item:Magnetos|CHECK both are on BTH
sw_item:Fuel Pump|OFF
sw_item:Tailwheel|UNLOCKED FOR TAXI
sw_item:Flaps|UP
sw_item:Mixture|AUTO RICH
sw_item:Throttle|800-1000 RPM to Warm up (Oil >50°) then 1000 RPM

sw_checklist:TAXIING
sw_item:Brakes|Checked

sw_checklist:BEFORE TAKEOFF CHECKLIST
sw_item:Mixture|AUTO RICH
sw_item:Propeller Control|FULL INCREASE
sw_item:Trim|SET FOR TAKEOFF (see Control panel)
sw_item:Flaps|UP (1/4 FOR SHORT FIELD)
sw_item:Cowl Flaps|ON TRAIL
sw_item:Landing Lights|ON
sw_item:Pitot Heat|ON
sw_item:Fuel Pump|ON

sw_checklist:LINED UP 
sw_item:Tailwheel|LOCKED

sw_checklist:TAKEOFF (sea level)
sw_item:Power|SET
sw_item:40 knots|Lift tail
sw_item:85 knots|Rotate
sw_item:100 ft|Landing Gear RETRACT
sw_item:300 ft|Landing Lights OFF (Ctrl+L)
sw_item:Flaps|UP
sw_item:Climb Throttle|45 MAP
sw_item:Climb Prop Pitch|2350 RPM
sw_item:Climb Airspeed|120-130 KIAS
sw_item:Mixture|AUTO RICH


sw_checklist:AFTER TAKEOFF CHECKLIST (Passing 1000 ft AGL)
sw_item:Gear|UP
sw_item:Flaps|UP
sw_item:Landing lights|OFF
sw_item:Fuel Pump |OFF
sw_item:Climb power|SET

sw_checklist:CRUISE
sw_item:Throttle|GREEN MAP
sw_item:Propeller Control|GREEN RPM
sw_item:Mixture|AUTO LEAN
sw_item:Cowl Flaps|near CLOSED (SHIFT+CTRL+C x 4)

sw_checklist:BEFORE LANDING CHECKLIST
sw_item:Rate of Descent|200 FPM
sw_item:Mixture|AUTO RICH
sw_item:Propeller Control|2150 RPM
sw_item:Cowl Flaps|ON TRAIL
sw_item:Fuel Pump (Main or Aux|ON
sw_item:Landing Lights|ON
sw_item:Cabin signs|ON
sw_item:Flaps 121 KIAS|1/4
sw_item:Gear|DOWN
sw_item:Tail Wheel|LOCKED
sw_item:Airspeed at Threshold|85

sw_checklist:BEFORE RUNWAY EXIT
sw_item:Tailwheel|UNLOCKED

sw_checklist:AFTER LANDING CHECKLIST
sw_item:Cowl Flaps|OPEN
sw_item:Flaps |UP
sw_item:Landing Lights|OFF
sw_item:Pitot Heat|OFF
sw_item:Fuel Pump (Main or Aux|OFF
sw_item:Trim|ZERO
sw_item:Tail Wheel|UNLOCKED

sw_checklist:SHUT-DOWN CHECKLIST
sw_item:Mixture|IDLE CUTOFF
sw_item:Magnetos Master|OFF
sw_item:Tailwheel|UNLOCKED
sw_item:Parking Brakes|SET
sw_item:Chocks|SET
sw_item:Lights|OFF
sw_item:Inverter|OFF
sw_item:Avionics|OFF
sw_item:Generators|OFF
sw_item:Battery|OFF